|  |
| --- |
| **STANDARD OPERATING PROCEDURE**  **OF RAW MATERIAL EVALUATION CANTER** |

|  |  |  |
| --- | --- | --- |
| **Author** | | |
| Name | Iqra Najib | **Signature** |
| Designation | Assistant Manager R&D |
| Date | OCT 24,,2020 |
| **Review** | | |
| Name | Ali Raza Gohar | **Signature** |
| Designation | QHSC team lead |
| Date |  |
| **Approval** | | |
| Name | Shahid Sultan Butt | **Signature** |
| Designation | General Manager |
| Date | Dec 30,2019 |

## Purpose

To ensure the quality of the new arrival raw material meets the specs of the product

## Scope

This procedure is applicable to REC Department of liquid master batch division responsible for raw material testing.

## Responsible

## Assistant Manager R&D

## Procedure

New arrival of the raw material is informed by our store team to REC through email or through Performa in which material name and its Lot# is being mentioned by our store team. Then raw material is being checked in its relevant grade and series. Every raw material has its own testing procedure. If a raw material for example pigment it will be checked in all the series in which it is being used. Not in all the grades but in all the series (MaxFlow OM, MaxFlow AM, DPM, Polytint Series, MaxFlow SM series, Akrilux series. .Following are the procedures used for the evaluation of the raw material.

**Evaluation of New Arrival Material:**

For the evaluation of the new arrival pigment it will be checked in shade and processing.

1. Raw material will be checked in the relevant grade with the help of recipe provided by developer.
2. Material will be processed in 1 stage (mixer) for mixing grades and 2 stages (mixing and grinding) for non mixing grades, ease of processing will be observed as per standard formulation.
3. Testing parameters (viscosity, shade, Gloss) as per product line will be tested and compared with standard.
4. If all the parameters are within standard range then labels of approval are provided to store staff to be placed on approved lots,
5. If any parameter does not lie within standard range then the material is adjusted as per standard requirement. After adjustment labels of approval are provided to store staff to be placed on approved lots.
6. If it does not meet the specs of the product even after adjustment, Label of rejection is pasted on it, and inform purchase department about the material.