**Operational steps**

1. Switch on the power buttons of spray booth.
2. Ensure the Air compressor on and air pressure adequate for pump speed.
3. Ensure the exhaust fans are properly working.
4. Ensure the flow of water in interior side of spray booth is properly working.
5. Ensure the gun is properly clean.
6. Check the viscosity of the paint in ford cup and ensure its value with standard range.
7. Check the working of the gun on spare panel to check if it’s working properly.
8. Spray the paint on Mild steel panels with 2-3 coats.
9. Clean the gun after using with recommended material for preparing next batch.

**Precautions**

Always use lab coat, Gloves, Face mask and safety goggles when working in spray booth.

|  |  |  |
| --- | --- | --- |
| **Prepared by:** | **Reviewed by** | **Approved by:** |
| **QHSE Member** | **QHSC team lead** | **General Manager** |
|  |  |  |