1. **Operational Steps**
   1. Turn on the pH meter.
   2. Clean the knob/ electrode of meter and make sure it is properly cleaned.
   3. Dip the knob for approx. 30 sec in sample for readings and then check the readings.
   4. Range of the pH value of our products is 7-9. Read the readings accordingly.
   5. Clean the electrode with relevant material after using.
   6. After readings place the knob/ electrode in its cell.
2. **Precautions** 
   1. Check pH of the samples at room temperature.
   2. Wear gloves during operation.