1. **Operational Steps**
2. Wear your prescribed personal protective equipment (PPE)
3. Ensure the platform is dry
4. Connect the switch and pour sufficient quantity of water to immerse temperature coil in it
5. Switch “ON” the power supply and button on water bath main unit
6. Adjust the required temperature using set button and upward ▲ and downward ▼buttons.
7. Cover the lid and let the temperature maintain to required value in water bath
8. Place the container having material which temperature is to be maintained in water bath
9. Cover with lid to maintain temperature, Check the temperature with thermometer till required temperature is achieved.
10. Remove the material container.
11. Switch OFF the water bath from main panel and disconnect power supply
12. Drain water in empty container using flow pipe on side of water bath.
13. **Safety Precautions**
14. Ensure that you have put on the prescribed personal protective equipment (PPE)-Eye goggles, face mask and gloves.
15. Pour pure water in water bath
16. Do not switch on electrical switches with wet hands.
17. Ensure surroundings of water bath is clean
18. If the cable attached to the water bath is damaged, stop using it. Contact your supervisor or maintenance department
19. Do not put your hands or anything in the water bath while it is operational.
20. Do not touch temperature coil while heating
21. Always unplug the water bath before cleaning and after using.