1. **Operational Steps**
2. First of all switch on the oven.
3. Then set the temperature. i.e. 2200C
4. For testing pigments place the pigment/MB on the aluminum plate in to the oven.
5. Then allow heating the samples for 10min.
6. After that open the door and pick out the sample plate.

Note: clean the oven.

1. **Precautions**

Do not let it on.

|  |  |  |
| --- | --- | --- |
| **Author** | **Review** | **Approval** |
| **Signature** | **Signature** | **Signature** |
| Muhammad Yousaf | Ghulam Murtaza | Ahsan Abid |
| Assistant Manager REC | R&D Manager | General Manager Operations |