1. **Operational Steps**

* Clean the body structure of generator and also clean the filters of generator set.
* Check all the following things in generator:
* Water level check.
* Diesel level check.
* Oil level check.
* Charging of batteries should always be on
* Terminals of batteries should be clean.
* On working load (Impairs) checking.
* Coolant temperature check.
* Oil pressure check.
* Oil pressure temperature check.

1. **Precautions**

* All the staff should be aware of any malfunction in generator set process.
* Any issue regarding process flow should be dealt on time to avoid inconvenience.
* If any issue found in generator it should be stopped immediately and checked thoroughly.

**Note:**

* If any type of warning indicators shows display of generator than immediately inform H.O.D or shut down the generator.
* If generator is in operating mode staff on duty is not allowed to leave generator, otherwise fine will be imposed.

(H.O.D) Electrical Department

|  |  |  |
| --- | --- | --- |
| **Author** | **Review** | **Approval** |
| **Signature** | **Signature** | **Signature** |
| Arqam Sattar | Waqar Islam | Ahsaan Abid |
| Assistant Manager Electrical | Maintenance Head | General Manager |