**Operational Steps**

1. Use power of V 240-220 for oven.
2. Switch on the button.
3. Open the door my moving handle to right side.
4. Place the sample at the grill and close the door.
5. Set the temperature at touch panel.
6. Set the time at timer screen.
7. Temperature starts to increase and stops at the specific temperature which is set on touch panel.
8. Place your samples when temperature reaches to the set temperature.
9. After the specified time open the door and remove the sample form grill.
10. Switch off the power button and remove the switch from power supply.

**Precautions**

1. Use heat resistant gloves and mask during use
2. Use spatula for removing samples.
3. Use safety goggles during use.
4. Clean the oven after use.
5. Don’t work on electricity with wet hands
6. Enter your name, temp setting and time (from - to) at a paper and paste at oven door.
7. Place samples on trey for easy removal.
8. Ensure oven is at safe temperature while cleaning. Clean spillage if any

|  |  |  |
| --- | --- | --- |
| **Prepared by:** | **Reviewed by** | **Approved by:** |
| **QHSE Member** | **QHSC team lead** | **General Manager** |
|  |  |  |