**Operational Steps**

1. Use power of V 220-240 for oven.
2. Switch on the power button.
3. Open the door by moving handle to right side.
4. Set the required temperature at touch panel.
5. Temperature starts to increase and stops at the specific temperature which is set on touch panel.
6. Place your samples in sample tray when temperature reaches to the set temperature. Place the tray in oven
7. After the specified time, switch off the power button Open the door and remove the sample tray from grill.

**Precautions**

1. Use heat resistant gloves and mask during use
2. Use safety goggles during use.
3. Clean the oven after use.
4. Don’t work on electricity with wet hands
5. Enter your name, temp setting and time (from - to) at a paper and paste at oven door.
6. Place samples on tray for easy removal.
7. Ensure oven is off while cleaning. Clean spillage if any

|  |  |  |
| --- | --- | --- |
| **Prepared by:** | **Reviewed by** | **Approved by:** |
| **QHSE Member** | **QHSC team lead** | **General Manager** |
|  |  |  |