**Operational Steps:**

1. Weight all the materials in lab according to given formulation and put into DPM mixer pot.
2. Close the lid of pot properly and check lid belt is properly in contact with pot surface there should be no gap/empty space.
3. Fix the pot into DPM mixer machine properly and close the fixed angles on both sides tightly.
4. Place the protection stand along mixer machine and switch on the main supply push start button on machine and rotate knob for speed adjustment.
5. Turn off mixer from on/off button after the given time of mixing has been completed and remove pot from machine.

**Precautions:**

1. Mixer pot should be completely fixed into machine.
2. Do not remove the pot while machine is in operation.
3. Safety stand should be present along mixer side at the time of operation.
4. Use safety goggles, lab coat and safety gloves during operation.