1. **Operational Steps**

* All the workers should follow the 5 S’s plan which is very important in a workplace. The 5 S’s are:

1. Sort
2. Straighten
3. Shine
4. Standardize
5. Sustain

* Before using any of the machine, make sure that all the connections are correct and double check it to avoid issues.
* The workers should not use the machines with wet hands.
* Make sure that the cables and wires of the machines in the workshop are properly insulated.
* While using the sawn machine, make sure that the guard of wheel is properly installed and workers should wear goggles to save eyes and body from fire sparks.
* While using the lathe machine, the workers should wear goggles, safety gloves to save eyes and body from hot and sharp iron particles.
* While using the welding Plant, the workers should wear welding screen & gloves to save eyes, hands and body from fire sparks.
* After using any of the machine, make sure that the supply is turned OFF.
* The supply connections should be properly removed.
* While any working is going to work on height and below any moving part, safety helmet must be used.

1. **Precautions**

* All the staff should be aware of any malfunction in the machines in the workshop.
* Any issue regarding the machines should be dealt on time to avoid inconvenience.
* If any issue is found in any of the machines, it should be stopped immediately and checked thoroughly.
* All the staff should be careful while using any of the machines.

**Note:**

* If any type of malfunction produced in any of the machines, then immediately inform H.O.D or shut down the corresponding machine.
* If machine is in operating mode staff on duty is not allowed to leave that machine otherwise fine will be imposed.

H.O.D Maintenance Department

|  |  |  |
| --- | --- | --- |
| **Author** | **Review** | **Approval** |
| **Signature** | **Signature** | **Signature** |
| Arqam Sattar | Waqar Islam | Ahsaan Abid |
| Assistant Manager Electrical | Maintenance Head | General Manager |