**Disclaimer**

The information provided in this TDS is believed by Bin Rasheed colors and chemicals to be the accurate one and is given in good faith to facilitate the end users, however it is up to end user to make necessary test before using this product, his own way and to determine the suitability of the product for user's intended application or use. This information should not be taken as warranty and ultimate standard.



**MICROFIX**

**Technical Information**

**Description**

MICROFIX is water based binder free high strength pigment dispersions. MICROFIX dispersions are compatible with stock paste for textile screen printing inks. MICROFIX dispersions are manufactured without Alkyl phenol ethoxylated additives.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Product Code** | **Color** | **Viscosity** | **Specific Gravity** | **pH** | **Particle Size** | **Use** |
| **cP** |
| **R # 1274** | Red | 2000 ± 200 | 1.0 ± 0.1 | 7- 9 | ≤ 5 µ | Screen Printing |

**Application**

The main application field of MICROFIX is screen printing inks. It is recommended to check maximum dosage level and compatibility of MICROFIX in your system

\*Given value of viscosity is based on QC result just after production. The value can vary during storage due to structure build up of anti settling agents. It may be brought to its actual value after high shear mixing.

**BINRASHEED COLORS AND CHEMICALS MFG.COMPANY**

338A-Sunder Industrial Estate-Lahore

Tel: +92 - 42 - 111-100-000 Fax: +92 - 42 - 3636 - 8877

W: [www.binrasheed.com](http://www.binrasheed.com/) E: service@binrasheed.com